

Procedure to update the SNF file


1. Copy the attached file to the PecStar\Context\SNF folder.
2. Start the PecConfig.
3. Click on the site to check the **Device Type**. Update the PMC-630C SNF file as below:




1. Select the first device under the site, right-click on it and select **Import SNF File** from the pop-up menu.




1. Select the corresponding xxx-1 SNF file for the first device of the device type, and click **Open**.




1. The warning window appears. Select **Yes** to replace the same ID data.




1. Select the second device under the site, right-click on it and select **Import SNF File** from the pop-up menu.




1. Select the corresponding xxx-2 SNF file for the second device of the device type, and click **Open**.




1. The warning window appears. Select **Yes** to replace the same ID data.



1. Update the PMC-630A SNF file in the same way.



1. After all the PMC-630A and PMC-630C devices are updated, save the changes to database.



1. Restart the PecSCADA.

